|  |  |  |  |
| --- | --- | --- | --- |
| **Customer:** | Roxul USA, Inc. | **Location/Desc:** | Byhalia |
| **Address:** | 4594 Cayce Rd | **Performed by:** | Kevin W Maxwell |
|  | Byhalia ,MS 38611 | **Date:** | 04/28/2023 |
| **Job/Order#** | 150012 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Reason for call:** | Field balance | | |
| **Description of work:** | Performed field balance on mega watt fan.  Dropped vibration 75% Initial imbalance: 3 mil pk-pk Final imbalance: .7 mil pk-pk @ 800 rpm.  Well within spec for rpm and fan type. | | |
| **Equipment and material used:** | 7 large C clamp weights | | |
| **Recommended additional work:** |  | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Main Contact:** | justin parker | | |
| **Customer Signature:** |  | | |

