|  |  |  |  |
| --- | --- | --- | --- |
| **Customer:** | University of Memphis | **Location/Desc:** | Memphis |
| **Address:** | Physical Plant & Plannin | **Performed by:** | Joseph Schurtz |
|  | Memphis ,TN 38152 | **Date:** | 06/02/2023 |
| **Job/Order#** | 150345 |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Reason for call:** | Sheave was misaligned and the motor kept throwing the belts. | | |
| **Description of work:** | Adjusted bearing on fan as it was cocked, moved sheave inward on fan, aligned sheave on fan and motor, had to adjust motor base to get angularity correct | | |
| **Equipment and material used:** | Sheave alignment laser | | |
| **Recommended additional work:** |  | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Main Contact:** | Fabian | | |
| **Customer Signature:** |  | | |

